

**How to Use Color Retrieval Function?**

**How to Use Color Retrieval Function?**

**Description**


***Note:*** *This method is applicable to most of the scenarios encountered problems, if the method still cannot solve your problem, it is recommended to consult our Tech Support Team.*

<https://global.uniview.com/Support/Service_Hotline/>


**Operating Steps**

Configure step 1 and step 2 on camera web:

**Step 1**: Set SIP or UMD rule on camera web, such as cross line detection and choose “attribute collection”.



**Step 2**: Click “**Setup> Intelligent> Attribute Collection”** to enable attribute collection function.




**Step 3:** Trigger the cross-line alarm.

Search result on NVR web:

**Step 4:** Click **“Smart> VCA search”** on NVR web

choosing color to search result on NVR web, such as green upper garment.



Then the result would be shown as below:

